info@venturefabrication.in +91 99658 44115
HO: TS NO: 980 North 3rd Street, Pudukkottai
Our Expertise

# Commercial Premises

Multi-story steel skeletons, composite deck floors, and custom architectural framing for modern commercial properties.

## High-Rise & Low-Rise Commercial Steel

Commercial premises require rapid structural completion, maximum open spaces for customizable office layouts, and code-compliant fire safety. Steel frames allow for lighter foundations, larger column spans, and rapid floor-by-floor concrete pours using composite steel decking sheets.

We fabricate composite beams, box columns, custom trusses, and steel stairs for multi-story office buildings, strip malls, and mixed-use commercial centers. Our modeling team matches blueprints with MEP contractors to pre-fabricate service holes, minimizing field conflicts and modifications.

### Technical Standards

Material Standard | AISC 360 LRFD Design, ASTM A992 Grade 50 I-Beams
Decking Support | Composite steel floor deck (1.5", 2" and 3" profiles)
Connections | High-strength bolted joints (A325 / A490) or field-welded CJP
BIM Coordination | Full IFC model sharing for MEP clash detection

### Key System Benefits

- Open Floor Layouts: Long-span steel beams offer wide, column-free office layouts.
- Fast Tenant Occupancy: Faster assembly allows contractors to start interior works months ahead of schedule.
- Easy MEP Integration: Pre-punched beams let HVAC and electrical lines run smoothly through the frame.

Get a Quote for Commercial Premises
Featured Projects

## Commercial & Public Structures

Explore our custom engineered cinema auditoriums and multi-story institutional steel frames.

Commercial & Public

### Shanthi Theater

Cinema auditorium large-span roof truss and stadium seating structure.

View Case Study
Commercial & Public

### Sri Venkateshwara School

Multi-story school building structural frame and staircases.

View Case Study
View All Project Portfolio