info@venturefabrication.in +91 99658 44115
HO: TS NO: 980 North 3rd Street, Pudukkottai
Our Expertise

# Cine Theaters

High-rigidity tiered platform frameworks, screen supports, and acoustic steel enclosures.

## Specialized Cinema Auditorium Steelwork

Modern cinema halls and multiplex theaters require highly specialized steel structures. The design must accommodate steep tiered seating platforms, massive support trusses for projection screens and speakers, and acoustic decoupling joints that prevent sound transmission between auditoriums.

Venture Fabrications provides high-rigidity structural solutions for cine theaters. We fabricate light-gauge and heavy steel members for stadium seating raisers, structural frames for acoustic baffles, and heavy gallows brackets that securely anchor massive projector systems and IMAX screens.

### Technical Standards

Material Standard | ASTM A36, A500 Grade B Steel, AISI Cold-Formed Steel
Platform Frame | Light-gauge steel framing with structural plywood or metal decks
Acoustic Controls | Elastomeric decoupling joints & structural isolations
Screen Supports | Custom wide-flange truss frames for curved screens

### Key System Benefits

- Optimized Sightlines: Custom-calculated riser steel angles guarantee perfect viewing from every seat.
- Vibration & Acoustic Isolation: Elastomeric washers and isolated joints reduce structure-borne sound.
- Rapid Multi-Screen Setup: Standard modular riser decks are fast to assemble inside primary skeletons.

Get a Quote for Cine Theaters
Featured Project

## Executed Cinema Theater Projects

Take a look at our completed cinema hall structural steel frameworks and tiered auditorium trusses.

Commercial & Public

### Shanthi Theater

Cinema auditorium large-span roof truss, acoustic deck framing, and balcony tiers.

View Case Study
View All Project Portfolio