info@venturefabrication.in +91 99658 44115
HO: TS NO: 980 North 3rd Street, Pudukkottai
Our Expertise

# Road Safety Sign Boards

High-wind resistant highway gantries, overhead sign frameworks, and hot-dip galvanized safety board supports.

## Galvanized Highway Sign Structures

Road safety structures and overhead signboards are continuously exposed to severe weather, high wind velocity, and exhaust fumes. To prevent structural failure and rusting, these structures must be engineered with high safety coefficients and protected with heavy galvanization.

Venture Fabrications designs and fabricates standard and custom highway gantries, cantilever sign supports, and roadside sign brackets. Every structure undergoes hot-dip galvanizing in accordance with ASTM A123 standards to ensure a lifetime of service without structural degradation or maintenance.

### Technical Standards

Material Standard | ASTM A36, A500 Grade B/C Tubular Sections
Anti-Corrosion Finish | Hot-dip galvanizing to ASTM A123 (min 85-micron coat)
Wind Load Design | Engineered to resist wind speeds up to 150 mph
Connection Type | Spliced flange connections with galvanized Grade 8.8 bolts

### Key System Benefits

- Decades of Maintenance-Free Life: Hot-dip galvanizing ensures absolute protection against rusting.
- Certified Safety Factor: Built to meet strict AASHTO wind-loading safety standards.
- Precision Pre-Fit: Gantries are trial-assembled in our yard to ensure rapid roadside installation.

Get a Quote for Sign Boards
Featured Projects

## Executed Road Safety Sign Projects

Take a look at our hot-dip galvanized highway sign structures, cantilever gantries, and VMS display frames.

Road Safety / Signs

### SR Infra Road Safety Gantries

Hot-dip galvanized road safety gantry frames and signboard supports.

View Case Study
Road Safety / Signs

### Variable Message Sign Board (VMS)

Heavy-duty gantry and cantilever VMS structure installed in Kodaikanal.

View Case Study
Road Safety / Signs

### Double Arrow Chevron Signboard

3M high-intensity reflective chevron hazard marker with galvanized support post.

View Case Study
View All Project Portfolio