info@venturefabrication.in +91 99658 44115
HO: TS NO: 980 North 3rd Street, Pudukkottai
Our Advantages

# High Resistance

Ductile structural steel provides high resistance to seismic activities, extreme wind loads, and industrial fire safety hazards.

## Structural Ductility & Safety Integrity

Unlike brittle masonry or conventional concrete which can crack and fail suddenly under load, structural steel exhibits outstanding ductility. Under intense stress, such as earthquakes or high-velocity winds, steel absorbs energy by bending rather than fracturing, providing critical safety margins.

Venture Fabrications designs structures using advanced load-resistance factor design (LRFD). We verify that all seismic moment-frame connections, tension rod bracing, and anchor bolts comply with AISC seismic specifications, protecting your facilities against natural forces.

### Resistance Benchmarks

Seismic Performance | Designed with ductile moment frames for high-risk seismic zones
Wind Resistance | Engineered to resist category 5 hurricane wind loads (up to 160 mph)
Fire Resistance | Supported with intumescent coatings for 1-hour to 4-hour fire ratings
Testing Standard | Non-destructive testing (NDT) on all critical moment welds

### Key Safety Advantages

- Earthquake Safety: High ductility absorbs seismic vibrations, preventing structural collapse.
- Hurricane Wind Load: Cross-bracing systems redirect high lateral wind forces to the foundation.
- Corrosion Protection: Industrial galvanizing prevents rust degradation in harsh chemical settings.

Get a Structural Assessment